**ISO TANK Kilnojamos talpos**

**(ISO TANK Portable tanks)**

Naujai statomam įrenginiui reikalingos talpos pastoviam alyvos laikymui.

Reikalingos savybės:

1. Talpa mažiausiai 20000ltr (gali būti daugiau).
2. Elektrinis šildymas
3. Lygio matuoklis (vizualinis ir elektrinis)
4. Tinkamumas EX zonai: ZONE 2 GAS GROUP IIA, TEMP. CLASS T3
5. Nurodykite, koks bus pajungimas, pagal kurį projektuosime vamzdynus ir prijungimus prie konteinerių.
6. Reikalingas talpų kiekis: 3 vnt.

Alyvos duomenų lapas, kuri bus laikoma talpose, pridėtas.

Pateikti pasiūlymą ir pardavimui ir nuomai.

Pavyzdinė nuotrauka:

A newly built facility requires tanks for permanent oil storage.

Required features:

1. Capacity: at least 20000 Litres (may be more).
2. Electric heating
3. Level gauge (visual and electric)
4. Applicable to EX zone: ZONE 2 GAS GROUP IIA, TEMP. CLASS T3
5. Indicate what kind of connections will be (we will then design the pipelines / connection to the containers).
6. Required number of tanks: 3 pcs.

Oil datasheet that will be stored in the tanks is attached.

Submit an offer for both sale and rental.

Example photo: