**Technical requirements for LOTO devices Annex No.1**

| **Description** | **Sample device** | **Purchase quantity (pcs.)** | **Engraving** | **Description** | **Notes Supplier shall submit proposal together with documents (certificates, descriptions, etc.) proving the conformity of devices with the above technical requirements).** |
| --- | --- | --- | --- | --- | --- |
| Locks (green)  670508000075 | Zenex safety padlock green S31GRN - S31KAGRN (manufacture Master Lock) | **1233** | G0001  G3600 | 1. Resistant to corrosion, chemicals, the housing is resistant to ultraviolet rays.  2. Suitable for outdoor use.  3. Each lock requires one key.  4. The side surfaces of the housing must have a clearly visible lock identification number of at least 4 mm in height, and a similar identification number must be on the lock key.  5. Suitable for use in potentially explosive environments (zone 2). |  |
| Locks with cables  (green color)  670508000076  670508000077 | https://cdn.webshopapp.com/shops/34658/files/50305286/brady-nylon-safety-padlock-green-with-cable-146127.jpg?_ga=2.180271140.1892978014.1557485745-296799959.1551882051  Nylon safety padlock green with cable 146127 (manufactured by Brady) or similar | **280**  (with 200 mm cable) | 1. Resistant to corrosion and chemicals, housing resistant to UV rays.  2. Suitable for outdoor use.  3. Each padlock must have one key.  4. A well visible identification number (at least 4 mm high)  must be inscribed on the sides of the padlock.  the same number must be inscribed on the padlock key.  5. Suitable for use in potentially explosive atmospheres (zone 2). |  |
| **404**  (with 400 mm cable) |  |
| Padlocks  (blue color).  670508000078 | https://cdn.webshopapp.com/shops/34658/files/26002717/master-lock-zenex-safety-padlock-blue-s31blu-s31ka.jpg?_ga=2.45591975.2082754372.1557732246-296799959.1551882051  Zenex safety padlock blue S31BLU - S31KABLU (manufactured by Master Lock) or similar | **171** | B0001  B0230 | 1. Corrosion resistant, UV resistant  2. Each padlock must have one key.  3. A well visible identification number (at least 4 mm high)  must be inscribed on the sides of the padlock  the same number must be inscribed on the padlock key. |  |
| Group lockout boxes  670524000031 | D:\DATA\EgidijusL\Pictures\abus-safety-redbox-group-lockout-b835.jpg  Safety Redbox group lockout B835 (manufactured by ABUS) or similar | **115** |  | 1. Wall mounted box for padlock keys.  2.Corrosion resistant, with robust carrying handle.  3.The cover of the box must have slots for up to 12 keypads. |  |
| Lockout devices for valves  670508030023  670508020022  670508020024 | D:\DATA\EgidijusL\Pictures\master-lock-lock-out-cable-s806.jpg  Lock-out cable S806 (manufacturer by Master Lock) or similar | **219**  (cable length – 61 cm) |  | 1.Adjustable flexible cable with an integrated safety  lockout hasp to cinch the cable tight.  2. Resistance to corrosion and chemicals.  3. Suitable for outdoor use.  4. Safety lockout hasp with 4 lockout holes.  5. Suitable for use in potentially explosive atmospheres (zone 2). |  |
| **464**  (cable length – 91 cm) |  |  |
| **151**  (cable length – 122 cm) |  |  |
| Lockout devices for blinds  670508020016  670508020003  670508020017 | Blind Flange Lockout Device,  Red/Black/Silver,  0.750 in to 1.125 in Nut Dia.Blind flange lockout device, S3922-S3923-S3924, (manufactured by Master Lock) or similar. | **750**  (bolt nut 19 mm – 28.5mm) |  | 1.Device fully conceals flange bolts preventing unauthorized access, covers and blocks out nuts.  2. Resistant to corrosion and chemicals.  3. Suitable for outdoor use.  4. Suitable for use in potentially explosive atmospheres (zone 2). |  |
| **405**  (bolt nut diameter 33 mm – 48 mm) |  |  |
| **68**  (bolt nut diameter 52 mm – 70 mm) |  |  |
| Lockout station  670524000030 | D:\DATA\EgidijusL\Desktop\BDS-29 2019_02_07\LOTO priemonės\abus-lockpoint-starter-set-77966.jpg LockPoint starter set 77966 Options: LockPoint + Chassis manufactured by ABUS) | **16** |  | Lock Point mobile safety center. |  |
| Storage baskets for LOTO devices  670524000032 | https://cdn.webshopapp.com/shops/34658/files/175208558/abus-lockpoint-basket-77948.jpg?_ga=2.33345854.1672820547.1552466112-296799959.1551882051  LockPoint basket 77948 (manufactured by ABUS) | **26** |  | Storage baskets for LOTO devices are affixed to the safety center Lock Point. |  |
| Padlock rails  670508020018 | https://cdn.webshopapp.com/shops/34658/files/175434092/abus-lockpoint-padlock-rail-77947.jpg?_ga=2.59101485.1672820547.1552466112-296799959.1551882051  LockPoint padlock rail 77947 (manufactured by ABUS) | **89** |  | Padlock rails are mounted on the Lock Point. |  |
| Key cabinet  670524000035 | https://cdn.webshopapp.com/shops/34658/files/12903398/master-lock-key-cabinet-7125d.jpg?_ga=2.133454921.631523815.1580719697-2070429430.1572516622Key cabinet 7125D  (manufactured by Master Lock) or similar. | **3** |  | Including 2 keys, key holders, installation fittings.  Size: 272 x 311 x 76 mm  Maximum number of keys: 60 |  |
| Padlocks  (yellow color)  670508000079  670508000085 | https://cdn.webshopapp.com/shops/34658/files/11822233/master-lock-zenex-safety-padlock-yellow-s31ylw-s31.jpg?_ga=2.106881536.2082754372.1557732246-296799959.1551882051  Zenex safety padlock yellow S31YLW - S31KAYLW (manufactured by Master Lock) or similar | **20**  **+70** |  | 1. Resistant to corrosion and chemicals, housing resistant to UV rays.  2.Suitable for outdoor use.  3.Each of these padlocks must have 5 keys suitable to unlock any padlock.  4.Suitable for use in potentially explosive atmospheres (zone 2). |  |